# Our Machine Products

### Conventional Milling

### Milling Machine Specification

TABLE
Sr. No. | Table | M-1 | M-11/2 | M-2 | M-3
--- | --- | --- | --- | --- | ---
1 | Table width & lenght | 230 x 1050 | 250 x 1070 | 280 x 1270 | 310 x 1450
2 | T-slot | 3 | 3 | 3 | 3
3 | Distance between T Slots | 52 MM | 56 MM | 67 MM | 78 MM
3 | T Slots Size | 16 MM | 16 MM | 16 MM | 16 MM
AXES TRAVEL
A | Table Travel Longiinal | 540 MM | 560 MM | 660 MM | 735 MM
B | Cross Travel | 190 MM | 230 MM | 255 MM | 310 MM
C | Knee Travel | 350 MM | 400 MM | 560 MM | 600 MM
FEEDS
A | Table Feeds | 3 | 3 | 3 | 3
MAIN SPINDLE
A | Spindle taper | ISO 40/45 | ISO 40/45 | ISO 40/45 | ISO 40/45
B | Spindle speeds RPM | 6 Speeds 50-700 | 6 Speeds 50-700 | 9 Speeds 40-1050 | 9 Speeds 40-1050
C | Cutting airbor | 25.4 MM | 25.4 MM | 32 MM | 32 MM
POWER
A | Motor | 2 HP 960 RPM | 2 HP 960 RPM | 5 HP 1440 RPM | 5 HP 1440 RPM
B | Coolant pump | 0.10 HP | 0.10 HP | 0.10 HP | 0.10 HP
SPACE REQUIRED
A | Lenght | 980 MM | 1000 MM | 1500 MM | 1600 MM
B | Width | 580 MM | 600 MM | 900 MM | 1300 MM
C | Height | 1600 MM | 1650 MM | 1850 MM | 2100 MM
D | Wight | 1000 kg | 1400 kg | 2200 kg | 3200 kg
NOTE : All the dimension are approximate

### Gear Hobbing Machine

#### Standard Accessories

1. Set of Change Gears (Feed/Differential/Index)
2. Hob Arbor
3. Work supports
4. Coolant System
5. Work Arbor
6. Machine lamp 24V

### GEAR HOBBING Machine Specification

MODEL HM 7 (All demision in mm)
Capcity |  |  | Work Table |
--- | --- | --- | --- | ---
Max Module | 7 |  | Dia of Gear | 550
Max. Diameter | 500 |  | Bore | 110
Min. Number of Teeth | 6 |  |  |
| Work Arbor |  |  | Hob Head |
Mounting Taper | 150, 40 |  | Setting for helical gear | 43
Max. Lenght of Job |  | Hob Cutter Size |
(a) Over the work Arbor Housing | 500 | Max. Dia | 120
(b) Through the Table Bore | 1000 | Max. Lenght | 127
Hob Arbor |  |  | Power |
Diameter | 32 |  | Main Driver Motor | 3.75 KW
Mounting Taper | MT4 |  | Rapid Traverse Motor | 0.75 KW
|  |  | Coolant Motor | 0.09 KW
Speed & Feeds |  |  | Weight |
Number of Hob Spindle Speeds | 9 |  | Net Wt. | 3000 kg

#### SPM Milling Machine

#### SPM Milling

#### Key Sloting Machine

#### Drilling Machine

#### Multi Spendle Drilling Machine

#### SPM Drilling Machine

#### Facing Machine

#### SPM Milling For Gear & Reamer Cutting